# quadEM Package Configuration

## xf02id1-ioc1 (quadEM-1)

|  |  |  |  |
| --- | --- | --- | --- |
| Package | | | Version |
| quadEM | | | R7-0.1 |
|  | ipac | | 2-13 |
| busy | | 1-6-1 |
| seq | | 2-2-1 |
| autosave | | 5-7-1 |
| sscan | | 2-10-2 |
| calc | | 3-6-1 |
| deviocstats | | 3-1-13 |
| epics-base | | 3.14.12.5 |
| areaDetector | | 2-5 |
|  | busy | 1-6-1 |
|  | autosave | 5-7-1 |
|  | calc | 3-6-1 |
|  | seq | 2-2-1 |
|  | deviocstats | 3-1-13 |
|  |  |  |
|  | |  |
|  | |  |

? areaDetector-R2-5 is incompatible with asyn-R4-30?

## xf28idc-ioc1

|  |  |  |  |
| --- | --- | --- | --- |
| Package | | | Version |
| quadEM | | |  |
| quadEM depends on: | ipac | |  |
| busy | |  |
| seq | |  |
| autosave | |  |
| sscan | |  |
| calc | |  |
| deviocstats | |  |
| epics-base | |  |
| areaDetector | |  |
|  | busy |  |
|  | autosave |  |
|  | calc |  |
|  | seq |  |
|  | deviocstats |  |
|  |  |  |
|  | |  |
|  | |  |